**DETAILS:**

* **Class:** Generators
* **Stock No.:**
* **Year of manufacture:**
* **Hours:**
* **Location:**
* **Price:** $ AUD (Excl GST)

**OPEN SKID DIMENSIONS:**

* **Length (mm):**  6,060 mm
* **Width (mm):**  2,440 mm
* **Height (mm):**  2,900 mm
* **Weight (Kg):**  16,000 kg

**DESCRIPTION:**

* Heavy duty, rental spec, sound attenuated to 85 dBA at 1 meter containerised, diesel generator
* Caterpillar 3412, twelve cylinder, V form, diesel engine
* Integral 1,350 litre daily fuel tank with bypass valves for external supply
* Full remote start capable control panel with island mode or utility synch paralleling control
* Motorised, paralleling, 4 pole, output circuit breaker with earth leakage protection
* Lead acid start batteries with charge alternator and trickle charger
* Permanently installed in a 20’ ISO container with internal lighting
* Fully bunded container to 110% of total fluid capacity
* Rated output 600 kW, 750 kVA, 50 Hz. 415V, 3 phase
* Rated current at 0.8 power factor 1,043 amps
* Ready to run and fully load tested.

**Call us on 1800 062 210**